    << PloComp >>
    Multi HPGL/Vector/Image file overwrite Viewer English
                       Copyright (C)1995-2026 Isoplotec Corporation
--------------------------------------------------------------------------
1. Outline

  PloComp is viewer which displays, prints and carries out data conversion 
of view file (HPGL,HPGL/2,HP RTL,PDF,DXF,DWG,GERBER,NC-drill,IGES,SXF,EMF,
TIFF,JPEG,Bitmap,PCX,FPX,GIF,PNG format) which works on Windows 7, 8, 10 and 
11 (contain 32Bit and 64Bit). PloComp has about the same powerful input and 
edit function as 2D-CAD, view file is read, addition editing and new drawing 
creation enable. It piles up or arranges and can display maximum of 20 file. 
Then, the drawing mode of Copy, Merge, and mirror ON/OFF in file 
unit can be chosen. It becomes enabling to see multi-file in piles or to 
confirm place where figures between multi-files differ by different colors 
of this function. Cloud shape region mark can be added to place with 
difference of two drawing. Rotation and grid display enable. Color, line 
width, display ON/OFF, and background color can be set up to pen. Color/black 
and white, line width variable / fixed change enables to all the pens. 
The contents of display can be copied to clipboard by color and black and 
white. The contents of display can be outputted to HPGL plotter, Windows 
printer,PDF,DXF,DWG,IGES,SXF,EMF,TIFF,JPEG,Bitmap,PCX,FPX,GIF, and PNG file.
 Coordinates, distance and angle for two points, line width, and distance and 
angle between lines can be measured. Line connected with line can be searched.

[About copyright]
  PloComp is developed based on "SXF common library Ver.3.xx."
Copyright of "SXF common library Ver.3.xx" belongs to Information-technology 
Promotion Agency, the Ministry of Land, Infrastructure and Transport, JACIC, 
and OCF.

--------------------------------------------------------------------------
2. Installation
  When you start PloComp to the 1st time, or when you enter password, user 
account should be "Administrator".

Step 1: Uninstall the earlier version of PloComp (see Section 4 below)
        before installing the new version.

Step 2: Create a temporary directory such as \Temp\PloComp.

Step 3: The new version is compressed in the ZIP file PLOCOMPxx.ZIP.
        Using WinZIP or a similar utility decompress PLOCOMPxx.ZIP into 
        the temporary directory created in Step 2.

Step 4: Explorer is started and SetupPloCompE.exe in folder of Step 2 
        clauses is double-clicked.

Step 5: Follow directions displayed on the screen.
        Our product has been virus checked.
        When "Windows protected your PC" is displayed at the time of 
        installation,
        if there is only "Don't run" or "OK" button, please click 
        "More info" and press "Run anyway" button.

Step 6: The program will now be installed automatically.

Step 7: In order to open compressed graphic files LZH or ZIP format in
        PloComp, the following files must be in next directory.
           for LZH files: UNLHA32.DLL;
           for ZIP files: UNZIP32.DLL.
        32Bit OS ... C:\Windows\System32 folder
        64Bit OS ... C:\Windows\SysWOW64 folder
        These files can be downloaded from the Internet home page.

Step 8: To input and output DWG files, it is necessary to separately 
        obtain and install the following "ODA File Converter".
        "ODA File Converter" is free software for DWG-DXF conversion 
        provided by Open Design Alliance and can be obtained from the 
        following Internet HP.
          https://www.opendesign.com/
        Click "ODA File Converter" in DEMO at the bottom of the page, 
        and download the installation file by clicking the following 
        installation file in Download on Windows Platform.
         - Windows XP or later (x86): "ODA File Converter for Windows x86"
         - Windows 7  or later (x64): "ODA File Converter for Windows x64"
        Double-click the downloaded file in Explorer to install.
        Start PloComp, select "Set InputFile" menu, and enter the full 
        path of the file installed in "DWG-DXF Conversion Program" 
        on the lower left.
        Example: OS and "ODA File Converter" version change
        - For 64Bit Windows
          C:\Program Files\ODA\ODAFileConverter_title 20.12.0\ODAFileConverter.exe
        - For 32Bit Windows
          C:\Program Files (x86)\ODA\ODAFileConverter_title 20.12.0\ODAFileConverter.exe
        Note: The contents described here are subject to change by
              the Open Design Alliance.

Step 9: PloComp registered into Internet HP is always the newest 
        version.  Since it becomes impossible for old PloComp to 
        come to hand, please take the backup copy through this 
        downloaded software PLOCOMPxxx.LZH.  Delete the temporary 
        directories and their contents created inSteps 2 and 3.

Step 10: Please install the printer driver of something, in the case 
        that the printer driver is not installed. 

Step 11: When outputting EMF file, it is necessary to set the following 
        settings of Windows to the initial values.
        "Start" "Settings" "System" "Display" "Scale and layout" 100%(initial value) 

--------------------------------------------------------------------------
3. After Installation

(1) Program folder
  PloComp program is in installation destination folder specified at 
the time of installation.
  It is the next folder if it installs by default.
    32Bit OS:
    C:\Program Files\Isoplotec\PloComp
    64Bit OS:
    C:\Program Files (x86)\Isoplotec\PloComp
  Please do not correct file in this folder.
(2) Configuration file folder
  PloComp configuration file and sample HPGL file are included in the 
next folder. 
  "username" is Windows account name.
    C:\Users\username\AppData\Local\Isoplotec\PloComp

--------------------------------------------------------------------------
4. Uninstalling

  It can be uninstalled using the Windows Control Panel [addition and 
deletion of program]: select PloComp from the scrolldown list and push 
 [Uninstall].

 And please delete configuration file in 3. (2) by Explorer. 
--------------------------------------------------------------------------
5. License agreement
   By install this software and using, customer is accepted to that is 
   restrained to the clause of this contract document.

(1) Copyright
   Isoplotec Corporation (below say the copyright holder ) has all 
   rights including the copyright of the software execution file, 
   program, and documentation. It is forbidden to convert this 
   software without the copyright holder's permission.

(2) License
   The customer installs 1 copy of this software only in 1 computer and 
   can use. This software cannot be operated remotely.

(3) Transferring, lending of the license 
   User is forbidden to transfer and lend the software to a third party.

(4) Guarantee of quality
   The copyright holder establishes the gratuitous use periods in the 
   customer evaluates the function and quality of this software for, 
   30 days. The copyright holder will accept information about defects 
   in the Software from customers for three years from the release date 
   of the latest version and will make efforts to correct the defects, 
   but is under no obligation to do so. 

(5) Upgrade 
   The customer must acquire the license of this software of the upgrade 
   version by the copyright holder, to use this software of the upgrade.  
   The upgrade version says case that the left column moves up from the 
   1st decimal point place of the version number of this software.  

(6) Exemption from Obligation
   Even in any case, the copyright holder shall not take the 
   responsibility at all regarding any other damage (including without 
   limitation, special, incidental, consequential, or indirect damages 
   for personal injury, loss of business profits, business interruption, 
   loss of business information, or any other pecuniary loss)that happen 
   from as a result that this software is used, or as a result that it 
   was not able to use this software.  Even if the copyright holder has 
   been advised of the possibility of such damages.  Even in any case, 
   the responsibility of the copyright holder makes the amount that the 
   customer paid out actually to the software the upper limit.

(7) Cancellation 
   In the case that the customer broke the clause or condition of this 
   contract document the copyright holder can cancel this contract 
   without injuring other rights.  In this case, the customer must 
   nullify all the reproduction things of this software.  

--------------------------------------------------------------------------
6. Licensing fee

   This software is shareware.

   When used 30 days or more from installation, please remit the next 
   licensing fee.
   Furthermore, please also pay remittance charge of PayPal.

   Licensing fee is                90.00 US$ / license

   When order from Japan, it is as follows.
      9,900 yen / license (tax included)
      However, it is only remittance to "Mizuho Bank Ltd.".
      Then, bank charge $28US is unnecessary and remittance charge is 
      remitter's charge.

STEP-1
   Please pay by PayPal.
   In PayPal, it can pay with credit card.
   Credit card payment enables at the next HP.
      https://www.isoplotec.co.jp/eplocomp.htm#Licensing fee
   Please carry out following HP reference about PayPal.
      https://www.paypal.com/
   Please remit to the following address in PayPal.
      isoplotec@isoplotec.co.jp

   Remittance to the next bank can also be paid.

    Bank name: Mizuho Bank, Ltd.
    Bank-/SWIFT-code: MHCBJPJT
    Bank address: Tokyo, Japan
    Bank Shop number: 128
    Bank Shop name: Fuchu branch office
    Account number: 1006122
    Subscriber name: Isoplotec

   In this case, please pay remittance charge of bank shown below 
   instead of remittance charge of PayPal.
   Please pay your bank charge.
   Furthermore, in addition to charge of license, please send our bank 
   charge $28US.
   Therefore, remittance amount of money is 
      90.00US$ * Order number + 28.00 US$
   For example, when the number of orders is 1, it is 118.00 US$.

STEP-2
   Send an email request for a order sheet as shown below.

Email format:

To: Isoplotec Corporation
     E-mail address: isoplotec@isoplotec.co.jp

Contents:
  Order sheet
  1. Soft name:              PloComp (English)
  2. Soft version no.:       12.0
  3. Order quantity:           1
  4. Company name:
  5. Offer person name:
  6. Offer person E-mail ID:
  7. Charge payment day:
  8. Charge payment amount:

STEP-3
   The copyright holder will email the password when payment of the
   registration fee has been confirmed.

STEP-4
   In order to enter password, when starting PloComp.exe, 
   it is necessary to carry out mouse right-click, 
   to take out pop up menu, and to select "Run as administrator".
   If it is within 30th after the installation, open PloComp and display
   'Version Information' dialog box with the menu 'Help'-'Version
   Information' and input the password. After the 30th day, input the
   password in the 'Set Password' dialog box which is displayed when
   PloComp is opened. Once this is done PloComp can subsequently be
   opened without the need of a password.

Note:
 - OS exchange or exchange of installation personal computer
  Even if you replace exchange of OS, or installation personal computer, 
  given password can release lock.
  However, the number which can install product in personal computer 
  simultaneously must not exceed ordered number.

 - Revision up (rise of the 2nd place of decimal point of version number)
  Revision up is free of charge.
  You can download new revision software from the internet HP and 
  you can reinstall.
  Previous password is effective.

--------------------------------------------------------------------------
7. Questions

   Please email questions about this software to Isoplotec Corporation.
   E-mail address is "isoplotec@isoplotec.co.jp".

   Internet HP
     https://www.isoplotec.co.jp/ehp.htm

--------------------------------------------------------------------------
8. Related products

(1) HPGL/Vector/Image Viewer  PloView

    The function difference with PloComp can display only one drawing 
    files.

(2) HPGL/Vector/Image printer continuation output program PloCon

    This is a version of PloView without the screen display, used for
    printing. It can be used to print multiple files continuously.

--------------------------------------------------------------------------
9. PloComp history

Ver.3.44 July 1, 2001
   (1) File open dialog changed to style of Explorer, permitting the
       opening of a network computer file.
   (2) The preview function added for printer/plotter output.
   (3) Support for IW (Input Window) command added
   (4) Support for FT (Fill Type) command added
   (5) Output area can be specified for TIFF image file output and a PDF
       file output; output file name can be edited.
   (6) TIFF image output enabled without opening of TIFF editing program.
   (7) Windows FONT characters can be used for TIFF and PDF output.
   (8) Character style can be specified with a standard font and an
       alternative font commands, respectively.
   (9) Improved method of calculating drawing size of arcs.
  (10) Program remembers output printer settings.

Ver.3.46 August 12, 2001
  (1) Several obstacles were modified.

Ver.3.5 September 22, 2001 - October 15, 2001
  (1) Support for DXF file output 
  (2) Support for JPEG image file output
  (3) Support for Bitmap image file output
  (4) The PDF file output function was improved to become small the PDF 
      file size since before in the case of the HPGL file where is using 
      many circulars or polygon form.
  (5) Improved to display normal even the HPGL data of the circular of 
      the radius zero, the real number coordinate that should are integer 
      coordinate.
  (6) The line of width of edge department form is able to be displayed 
      in the circle, square, or triangle, by that corresponded to the LA 
      command (the line attribute command). 
  (7) When PDF, TIFF, DXF, JPEG, Bitmap are output it is possible be 
      designated the unfilled space.  

Ver.3.6   January 3 2002 - March 21 2002
  (1) Added search function of text.
  (2) Added length measure function between points.
  (3) Added length measure function between lines.
  (4) Added Zooming ON/OFF of ZoomIcon.
  (5) Unless Imaging for Windows of Windows attachment was installed 
      conventionally, normal starting of the PloComp was not carried out.
      Even if Imaging for Windows was not installed this time, it improved 
      so that it might move normally. Since Imaging for Windows is not 
      appended to WindowsXP, this correspondence is indispensable.
  (6) It corresponded to RO (coordinate system rotation command).
  (7) It enabled it to choose the right/center/left and the top/center/bottom 
      of the paper as plotting position at the time of Windows printer output.
  (8) It enabled it to choose the right/center/left and the top/center/bottom 
      of the paper as plotting position at the time of PDF output.
  (9) The file name is named and saved at the parameter file and it 
      enabled it to open it.
  (10) It corresponded to UC (User-Defined Character command).
  (11) Added function that ignore PC (pen color) command at SetPen menu.
  (12) Added function that ignore PW (pen width) command at SetPen menu.
  (13) Added function that ignore FP, RA, RR, WG (paint polygon, rectangle, fan)
       command at SetPen menu.
  (14) Added pen table at SetPen menu. The setting value such as the color, line
       width for each pen number are remembered. 

Ver.3.7  June 2, 2002
  (1) Added the function that is able to search the connection of the line. 
  (2) You can request the length of the total line that searched it in 1 clause.
  (3) PreView mode was added to the OpenFile dialog.
  (4) The function that displays the 1st HPGL file name that is setting up it 
      in the parameter file to the menu of Open Parameter File and Save 
      Parameter File was added.
  (5) The Display button was attached to Set Display ON/OFF dialog.  It is 
      displayed in the condition where the dialog opened, when you push this 
      button.
  (6) When the mouse cursor is moved on the check box of File1 from File10 of 
      Set Display ON/OFF dialog the HPGL file name is displayed with the hint.

Ver.4.0 November 23, 2002
  (1) The function to insert and edit the comment (the straight line, the 
      free curve, the rectangle, the long circle, text) was added.
  (2) It enabled it to change the connected line into the comment.
  (3) The HPGL data and comment data which are seen are made into the 
      attached file, and it could be made to carry out E-mail dispatch.
  (4) Expansion reduction is carried out with the mouse wheel, screen 
      movement is carried out by the on-drug of the middle button of the 
      mouse, and the whole was displayed in the double click of the middle 
      button of the mouse.
  (5) The pop up menu was displayed as the mouse right button.
  (6) The Window position and size at the time of PloView starting were 
      made to become last time the same as the time of the end.
  (7) The tool button of the PDF, TIFF, DXF, JPEG, and Bitmap output was 
      prepared.
  (8) It corresponded to the PJL format BZ (absolutely coordinates Bezier 
      curve) and BR (relative coordinates Bezier curve) command.

Ver.4.1 March 10, 2003
  (1) PDF output compressed by ZLIB was supported.
      Compared with the former, file size becomes small to 1/2 .. 1/9.
  (2) When output TIFF file, it corresponded to HPGL data with more large 
      drawing size, and more larger resolution compared with the former.
  (3) It enabled it to choose one of the folder which outputted last time, 
      or the open HPGL file folder at the time of PDF, TIFF, DXF, JPEG, and 
      Bitmap output.

Ver.5.0 October 11, 2003 - January 10, 2004
  (1) It corresponded to HP RTL (HP's Raster Transfer Language, image data).
  (2) The pen number corresponded to a maximum of 255.
  (3) It corresponded to IR (relative scaling point) command.
  (4) It enabled it to use No.0 pen.
  (5) The maximum number of HPGL file opened simultaneously was increased 
      from 10 to 15.
  (6) The maximum number of Window opened simultaneously was increased 
      from 5 to 15.
  (7) The mode which carries out "Displays in arranges" and "Displays in 
      piles" with Set-Display ON/OFF menu.
  (8) It corresponds to the shade level (net display) of painting out of 
      FT command.

Ver.5.1 March 7, 2004
  (1) Add an IGES file output function.
  (2) Add an EMF file output function.
  (3)  The file type of a TIFF file output was only GROUP4 conventionally.
      This time, un-compressing, CCITT RLE, GROUP3 1D, GROUP3 2D, 
      and PACKBITS are added.
  (4) In TIFF file output, only black and white corresponded 
      conventionally.  This time, it corresponds also to the color of 
      16 colors, 256 colors, and 16 million colors about the file type 
      of un-compressing and PACKBITS.
  (5) In JPEG and a Bitmap file output, only black and white corresponded 
      conventionally.  This time, it corresponds also to the color of 16 
      colors, 256 colors, and 16 million colors.
  (6) The kind of file was fixation conventionally in the OpensFile dialog.  
      This time, user can set up.  If the file extension which starts in 
      "*." is specified as the SelectFile column, it can register with a 
      "Kind of File" combo box.  It will be deleted if the same character 
      string is specified again.

Ver.6.0 May 30, 2004 - June 27,2004
  (1) The following function was added.
      TIFF, JPEG, Bitmap, PCX ,FPX, and PNG image file are read, and 
      displays, and outputs.
  (2) When the file which outputted HPGL through Windows printer driver 
      of HPGL output was read from WORD, Excel, etc., it repaired that 
      there was a case where image was coarse and color was amusing.
  (3) The printer setting button was added in the dialog at the time of 
      printer / plotter output.
  (4) The same zoom display function as Acrobat Reader was attached to 
      the zoom expansion display icon and the zoom reduction display icon.
  (5) When it changed into the state of "arrang display" by "display 
      ON/OFF setup", and printer, PDF, TIFF and JPEG, Bitmap, DXF, IGES, 
      and EMF are outputted, the mode which outputs all files collectively 
      was added.
Ver.6.0 August 18, 2004
  (6) It improved so that it might display and output in each drawing 
      size by "Displays in arranges".
  (7) Order of Window was made into the order of file No. when additional 
      deletion of the file was carried out in "Displays in arranges".
Ver.6.0 August 28, 2004
  (8) At the time of "Displays in arranges", conventionally, the comment 
      file of No.1 was displayed on all Windows, and has edited.
      It improved so that it could have a comment file separately for 
      every Window this time.
  (9) Although the conventional comment file was fixation at the file of 
      No.1 at the time of "Displays in piles", it improved so that it 
      could change in "Display ON/OFF" this time.
  (10) It expanded to 10.0mm that the maximum of pen width was 3.0mm in 
      "SetPen".
Ver.6.0 September 26, 2004
  (11) In TIFF, JPEG, and Bitmap output, the function of "Set Auto Scale", 
      "Set Output Scale", "Set Paper Size", and "Set Plot Position" was 
      added.
Ver.6.0 October 03, 2004
  (7) With the IGES output, the function to change correspondence of a 
      HPGL pen number and an IGES pen number was added.
  (8) The figure maximal domain and PS (plot size) command area can be 
      chosen for drawing size (area displayed when whole display 
      command is issued) in the dialog which opens file.
Ver.6.0 January 10, 2005
  (9) The pen number translation table translated into another pen number
      to the pen number of the inputted HPGL file by set-pen command was prepared.
  (10) By the set-pen command, it was named to the pen table.
  (11) By the set-pen command, the button to preview was prepared after the
      setup for the check.
  (12) The icon of a rotation display was prepared for the tool bar.
  (13) The pen table change icon was prepared for the tool bar.
Ver.6.0 April 24, 2005
  (14) Improvement in drawing accuracy
  (15) The abnormal end of rare conditions is repaired.

Ver.6.1 January 3, 2006
  (1) Length system of units (mm, cm, m, in, ft, yd) to be used can 
      be set up.
  (2) Use floating point of length system of units for display and 
      setup of coordinates and dimension.
      Setup of line width of former, for example, 0.3mm pen, was 
      0.01mm integer specification like 30. This can be specified as 0.3.
  (3) Support command which displays graph of HPGL shown below.
      XT (X-Tick): Drawing vertical scale
      YT (Y-Tick): Drawing horizontal scale
      TL (Tick Length): Scale length setup
      XA (X-Axis): Drawing X axis
      YA (Y-Axis): Drawing Y axis
      GR (Graph Reletive) : Drawing line graph of X-Y
  (4) Support AT (Absolute Arc Three Point) command and RT (Relative 
      Arc Three Point) command.
  (5) Line type corresponds to -1..-8(length self-adjustment), and 7
      (two-point chain line), 8(three-point chain line) and 99(line 
      type restoring) by LT(Line Type) command.
  (6) When line thickness surpasses 0.35mm, correspond to Line Joins 
      form (Mitered join, Miterd/beveled join, Triangular join, Rounded 
      join, Bebeled join, No join) and Miter Limit by LA 
      (Line Attributes) command.
  (7) It corresponds to mode which follows TR (Transparency Mode) command 
      of HP-GL/2 by setup of Draw Mode of file open dialog.
  (8) With DXF output, improve color, line type, up-and-down length of 
      dotted line and chain line, and line width so that it may become 
      the same as HPGL data.
      Color number which can be used was increased from 7 to 255.
      Line, arc, and circle are changed into polyline of DXF.
  (9) Some obstacles were repaired.
Ver.6.1 February 28, 2006
  (10) LZW became possible with TIFF output.

Ver.6.2 April 8, 2006
  (1) Difference of figure of two drawing files was found with 
      "request"-"change area" menu, and function to obtain change 
      area was added.
  (2) It enabled it to specify plural drawing files with parameter 
      at the time of PloComp starting.
Ver.6.2 June 25, 2006
  (3) In straight line of comment, and free form curve input, it improved 
      so that cloud mark form could be drawn.
  (4) When cloud mark was outputted to comment in request-change area, 
      cloud mark was conventionally approximated with polygon of free 
      form curve, but it was made cloud mark form of comment.

Ver.6.3 October 1, 2006
  (1) Thumbnail display function was added.
      "Page display", "thumbnail display", and "thumbnail and page 
      display" can be changed with display menu.
  (2) Since picture will disappear if it draws a picture with pen of 
      the same color as background color, setup of "Color is changed 
      when pen color is same color as background" can be performed 
      with set-pen menu.
  (3) Plural defect were repaired.
Ver.6.3 October 14, 2006
  (4) Preservation or deletion of thumbnail file can be specified with 
      "Set-Thumbnail" menu.
  (5) Display can be returned before a maximum of 10 times with "Display
      - Undo display" and "Display- Redo display" menu.
Ver.6.3 November 4, 2006
  (6) Floating tool bar which can move to four corners of Window and 
      possible to display ON/OFF was used.
  (7) The number of tool buttons was increased greatly and design of 
      tool button was improved.
Ver.6.3 February 12, 2007
  (8) When color number of drawing was made into single color by OpenFile, 
      it improved so that it might display by the specified color.
  (9) When DrawMode of image file was specified as Merge and Xor by 
      OpenFile, it was displaying in Copy mode in the past, but it was 
      made to display in the specified mode.
  (10) Function to open specified page of multi-page file was added.
      16 pages or more are available as specified page.
  (11) Method of opening specified page of multi-page file at PloComp 
      starting command line, and the method of skipping file number 
      and assigning drawing file were added.

Ver.7.00 August 16, 2007
  (1) It corresponded to Windows Vista.
  (2) It enabled it to use it by general user account of Windows.
  (3) Help was changed into HTML help.
  (4) Installer was changed.
  (5) Change of installation destination
      Installation destination was divided into program folder for 
      all user readings, and setting folder which can perform reading 
      and writing for every user.
  (6) It checked whether to have been administrator authority at the 
      time of password input.
  (7) Various bugs were repaired.
Ver.7.00 September 22, 2007
  (8) When character of Back Space was in LB (label) command, in the 
      past, ? was drawn. This time, it was made to carry out processing 
      of Back Space.
  (9) It corresponded to FR (frame delivery) command.

Ver.7.01 October 8, 2007
  (1) It enabled it to specify output scale with DXF output and IGES 
      output. In the past, scale was fixation in 1 time.
  (2) Resolution of PDF output was raised from 0.1mm to 0.001mm.
      In the past, it had become inaccurate figure, when it reduced 
      greatly and having been outputted.

Ver.7.02 November 3, 2007
  (1) Function of HPGL plotter output was improved.
      It sets up by plotter1.par and plotter2.par file.
    - Label can be outputted to character or line segment.
    - Circle can be outputted to circle or polygon.
    - Painting out can be outputted to painting out or line segment
      (hatching).
    - It corresponded to many commands of HPGL.

Ver.8.01 May 25, 2008
  (1) It enabled it to read PDF and EMF file.
  (2) Function which carries out data conversion to WMF, EMF, PS, SVG,
      XPS, HPGL, and PCL from PDF file was added.
  (3) Restriction of Windows font was lost at the time of PDF file output.
  (4) When PDF and EMF file were read, mode which displays font currently 
      used in the file was prepared.
  (5) It supported to CO (comment) command.
  (6) Progress bar was displayed at the time of thumbnail creation.
  (7) It was made for improvement in resolution and frame size data to
      be included with EMF output.

Ver.8.02 June 29, 2008
  (1) Although color operator of PDF output was only RGB in the past, 
      you could specify CMYK.
  (2) Overprint was supported with PDF output.

Ver.8.03 July 21, 2008
  (1) Font can be selected in comment text input and Chinese and Korean 
      can be inputted.
  (2) Dragging of Windows Font is made at the time of text input of 
      comment.
  (3) Indicate the character of Windows Font by mirror on screen.
  (4) Merge and Xor displaying of character of Windows Font can be 
      performed.
  (5) PDF and EMF containing character of Chinese and Korean can be 
      inputted.
  (6) One comment character of 255 or more characters can be inputted.
  (7) Character (mirror character) of minus character width can be 
      displayed by Windows Font.

Ver.8.04 September 1, 2008
(1) Improvement in the speed of displaying of image.
(2) When the black-and-white image is set by reduction, display by gray scale.
(3) It enabled it to read GIF and JPEG2000 of image file.

Ver.8.05 January 10, 2009
(1) When having set specific printer as "usually used printer" and it tried 
    to have opened PDF, there was case where error of "open error!code=1002" 
    was displayed and it did not open.
    It was made to open normally when printer driver which does not become 
    error was installed in others.

Ver.8.06 May 6, 2009
(1) WMF, PS, EPS, SVG, XPS, and PCL output were supported.
(2) When it converted into PS and EPS by "File"-"Convert PDF file", 
    it repaired that scaling was carried out to fixed form paper size, 
    and margin was made in the four corners.
    However, character is outside support except alphabetic character font.

Ver.8.07 Jan 9, 2010
(1) Registration / release function of file extension of relation was appended.
(2) Letter reading of EMF file was repaired.

Ver.8.08 Jan 20, 2010
(1) After turning OFF "Display comment Tool" with "Comment-Display comment Tool"
    menu and ending PloComp, it repaired terminate abnormally, if PloComp is 
    started next.
(2) It repaired that there were conditions that cooperation of "Comment-Display
    comment Tool" and "Comment-Dsiolay comment" menu was strange.
Ver.8.08 Jan 20, 2010
(3) Operation on Windows7 was guaranteed.
(4) It supported to UL (user line type) command.
Ver.8.08 Mar 06, 2010
(5) Some bugs were repaired.
Ver.8.08 April 06, 2010
(6) Some bugs were repaired.
Ver.8.08 April 24, 2010
(7) EMF file output and click board copy were repaired.
Ver.8.08 May 27, 2010
(8) The maximum number of pen number translation table was increased from 5 to 20.
(9) The maximum number of line connection check was increased from 20 to 200.
Ver.8.08 May 29, 2010
(10) The maximum number of pen table was increased from 5 to 20.
(11) The "Change all pen width to pen0" button in SetPen dialog was added.
Ver.8.08 June 9, 2010
(12) "Set"-"drawing origin" menu was added.
The drawing origin is movable by pointing out two points with mouse.
Ver.8.08 June 10, 2010
(13) When color number of image was 256 or more at PDF output of the drawing
     containing an image, in the past, it was reducing in 256 colors.
     It was made to output without reducing the color number this time.
(14) The icon for WMF, PS, EPS, SVG, XPS, and PCL output was prepared for
     main window lower left.
Ver.8.08 June 19, 2010
(15) When PDF and an EMF file read, it had not supported to clipping of
     complicated shape. It supported now.
Ver.8.08 July 11, 2010
(16) Displaying speed was raised at Windows Vista and 7.
Ver.8.08 July 15, 2010
(17) The automatic paper select function (A4 / A3/A2 / A1/A0, length/width) was 
     added with PDF, TIFF, Bitmap, Jpeg, WMF, PS, EPS, SVG and XPS, and a PCL 
     output.
Ver.8.08 July 23, 2010
(18) The accuracy of position at the time of PDF and an EMF input was improved.
Ver.8.08 July 28, 2010
(19) The reading speed of PDF and EMF file containing many characters was improved.
Ver.8.08 July 30, 2010
(20) PDF input-and-output problem of image data was repaired.
Ver.8.08 August 17, 2010
(21) PDF input-and-output problem of text data was repaired.
Ver.8.08 August 20, 2010
(22) Drawing size at the time of a PDF input was improved.
(23) Drawing size was displayed when it displayed.

Ver.8.09 August 27, 2010
(1) Optional feature of "Display procedure" (Momentary display/Sequentially display) 
    was appended in SetPen dialog.
    Displaying speed changes with "Display procedure" and combination of personal 
    computer hardware, OS kind, DrawMode, and drawing data.
    In Vista and 7, if it is not made Momentary display, displaying will become 
    quite slow.
Ver.8.09 November 1,2010
(2) The composition of an installer was changed.
Ver.8.09 December 16,2010
(3) It becomes error to read the file which carried out the PDF output by Adobe 
    Reader when the decimal point character of the real number is set as "," 
    with the control panel of Windows.
    It was repaired.
Ver.8.09 March 11, 2011
(4) It supported to DL (download character) command.
Ver.8.09 July 18, 2011
(5) Displaying improvement of color image.
(6) Magnification of drawing size in which color image output enables.
(7) Mouse wheel setting addition.
Ver.8.09 December 9, 2011
(8) Linkfile was opened by OpenFile Dialog.

Ver.8.091 February 06, 2012
(1) When having set up Correct Rate of Text Size by SetText other than 100%, 
    it corrected that character position of continuous LB (label) command had 
    shifted.
(2) It corrected so that the following character when CS (standard   character set) 
    command is set might be displayed correctly.
    CS3 '[' ==> '0'
    CS4 '\' ==> 'i'
(3) It enabled it to set PS (plot size) command initial value to option setting 
    tab of OpenFile dialog.
    In the case of HPGL file in which PS command and IP (scaling point P1, P2 
    input) command are not included, SR (relative character size) command etc. 
    which affect scaling point can be controlled now.
Ver.8.091 March 26, 2012
(4) Improvement of IGES output
(5) Improvement of big arc displaying
Ver.8.091 May 15, 2012
(6) With IGES output, when input and output file name were 60 or more characters, 
    IGES data corrected fault which becomes abnormal.
Ver.8.091 May 28, 2012
(7) In HPGL input, 1-byte katakana of the character set 43 of SD command and AD 
    command was supported.
(8) When C/R and L/F were in 1 byte of katakana character by LB command, it 
    repaired having displayed abnormal character.
(9) Function which transmits evaluation report by E-Mail was deleted.

Ver.9.00 January 10, 2013
(1) It supported to reading of two-dimensional DXF file (version is 
    AC1025 and equivalent to 2000/2000i/2002 in AutoCAD version).
(2) It supported to reading of GERBER file.
(3) It supported to reading of NC-drill.
(4) It supported to reading of two-dimensional IGES file.
(5) In addition to AutoCAD version GX-5 conventional correspondence, 
    DXF file output could newly be made to perform 2002 correspondences.
(6) In addition to conventional Bitmap, TIFF, and Jpeg, image output 
    supported to GIF, PNG, PCX, and FPX.
(7) Coordinates accuracy of internal processing was raised from 
    0.025 mm to 0.001 mm or less.
    Coordinates when it requests, and the minimum unit of length 
    were 0.001 mm from 0.01 mm.
(8) It was made to set up input file relations with set input file 
    menu. It enabled it to set up file extension for every file type.
    Extension set up here is displayed on "kind of file" of OpenFile 
    dialog.
    In the past, since file type and file extension's relation were 
    unknown, this is improvable although there was case where file 
    which PloComp is not supporting was selected and PloComp hung-up.
(9) Designation of extension which can be searched with set thumbnail 
    was stopped, and all the extensions registered by set input file 
    were used as extension searched with thumbnail.
(10) Pen number was displayed by dimension measurement between 
    request lines.
(11) Since various output parameters were common, output scale set 
    up with other outputs was used, and it may have outputted with 
    unexpected scale. Then, automatic scale and output scale memorized 
    setup for every output.
(12) Width of string to display was adjusted so that it might become 
    width specified by data.
(13) It supported to Windows8.
(14) "Multi-file auto select" check box was prepared in OpenFile dialog.
    If this is checked, it is only selecting one file and can select 
    automatically simultaneously plural files with name of conditions 
    shown below. Number of file name end becomes file number.
    - It exists in the same folder as selected file.
    - It is the same file extension as selected file.
    - File name leading character string of selected file is the same 
      as it, and ends of file name is numbers 1-15.
(15) Licensing fee was changed by change of exchange rate.
Ver.9.00 January 15, 2013
(16) The conventional "Momentary display" was changed into 
    "Momentary display 1" for display type with the "set "-" pen" menu, 
    and "Momentary display 2" was newly added.
Ver.9.00 March 13, 2013
(17) With PDF output, smearing away of mesh was carried out to coating 
     whose shade level is 100%.
     It was light-color-ized according to shade level.

Ver.9.01 May 2, 2013
(1) The next function was added with HPGL plotter output.
    - Add button into which plotter parameter file is edited.
    - It enabled it to select specification of output HPGL data from the 
      next three kinds by plotter parameter file.
         HPGL         : Simple functional vector
         HPGL/2       : Highly functional vector
         HPGL/2+HP RTL: Highly functional vector + image
(2) Five kinds of Text size candidates were prepared by comment attribution 
    setup.
    If Text size used well beforehand is registered into candidate, 
    Text height, width, and space can be collectively set up only by 
    selecting from candidate.
(3) Defect was repaired.
Ver.9.01 May 28, 2013
(4) Output of images, such as TIFF, JPEG, and BitMap of big size 
    (for example, double size of A0, black and white, 400DPI), repaired 
    defect to which scale becomes smaller than designation.
Ver.9.01 October 16, 2013
(5) It repaired abnormal, when GERBER file that starting point and 
    terminal point of arc correspond was read.
Ver.9.01 October 18, 2013
(6) The number of constituting points which can smear away surface was 
    increased.

Ver.9.02 October 25, 2013
(1) Since arc was displayed as G74 (quadrant ON) when GERBER file 
    without data of G75 (quadrant OFF) is read, abnormal arc was drawn.
    Then, it could be made to perform setup of G74 (quadrant ON) ON/OFF 
    in Set-Input file.
Ver.9.02 November 04, 2013
(2) Garbled characters of warning dialog (title and button) have 
    been improved.
Ver.9.02 December 05, 2013
(3) It repaired becoming system error by "DL character number;" of 
    DL (download character) command.
(4) When space character was after "CO" by CO (comment) command, 
    it repaired having become abnormal display.
Ver.9.02 December 17, 2013
(5) When there were big coordinates more than 2,147,483,647 HPGL Unit
    (53,687,091.175 mm) by HPGL data, it repaired that it was abnormal.
    In relation to this, the maximum coordinates which can be inputted 
    were limited to 214,748,364 HPGL Unit (5,368,709 mm).
Ver.9.02 December 22, 2013
(6) File was not opened when there was no '%ADD' command into GERBER file.
    This has been improved.
(7) File was not opened when + symbol was in top of XY coordinate value 
    of GERBER and NC file.
    This has been improved.
Ver.9.02 January 04, 2014
(8) When closed line was searched with "Request"-"Line connection search"
    menu, function of determine area was added.
(9) With "Request"-"Change area" menu, function of request for change 
    area in ZoomCopyArea was added.
    "All of Draw" and "Display outermost area" are selected, and if two 
    files which figure frame has shifted are compared, it cannot request 
    for change area inside figure frame.
    However, it will become enabling if "Zoom and Copy area" is selected.
Ver.9.02 January 22, 2014
(10) Improvement below "Request"-"line connection search" menu was carried 
    out.
    - Improvement in accuracy of line connection
    - Improve measuring abnormal area.
    - Scale can be specified.
(11) At the time of reinstallation, in the past, after uninstalling, 
    it needed to install.  Now, installer was improved and uninstallation 
    was set unnecessary.
Ver.9.02 February 10, 2014
(12) The 23..25th parameters were added to global section with IGES output.
(13) "Request - Surface search" function was added.

Ver.9.03 March 18, 2014
(1) Range corresponding to Windows Font was extended.
    - Support simplified Chinese character, the traditional Chinese 
      character, and Hangul alphabet character with DXF input and output.
    - Support mirror display of TrueType Font with Printer and Plotter output.
(2) Display of character with negative width and height(mirror display) 
    which uses Windows Font was repaired.
(3) When 1 byte and 2 byte character were intermingled by character input
    of comment, it repaired having displayed abnormal character.
(4) File extension of Plotter output was changed into ".hgl".
Ver.9.03 April 1, 2014
(5) MaskNotPen mode was added to DrawMode of OpenFile dialog.
Ver.9.03 May 26, 2014
(6) Repair AT (three-point arc) command of HPGL.
Ver.9.03 May 30, 2014
(7) Repair Request Change Area menu command. 
Ver.9.03 June 19, 2014
(8) Improvement of DXF input.
Ver.9.03 July 06, 2014
(9) Repair when "Initial of Line End Shape" was set to "square" by 
    SetLineProperty was performed.
(10) Character size was repaired, when Windows Font was selected by 
    SetText and 1 byte of ASCII character was displayed.
(11) Display of DV command has been improved.
(12) Function which can also distinguish difference of color in 
    Request-Change area serach was added.
    Since it had distinguished by black-and-white display in the past, 
    difference of color has not been recognized. 
    Now, function distinguished by display of 257 standartd colors or 
    display of 256 darawing colors of 256 or less colors was added.
(13) Color of line measured by Request-Length measurement between 
    lines was displayed.
    Color attribution can be seen if it clicks displayed color.
Ver.9.03 July 16, 2014
(14)Improvement of LB command of HPGL.
(15)Improvement of vector font display.
Ver.9.03 August 28, 2014
(16) Only one copy was printed even if it set print copies with set printer 
    by Windows 7 and 8. Then, it enabled it to set up print copies with 
    Windows Printer output of plotter setting dialog.

Ver.10.01 March 2, 2015
(1) Comment function was greatly improved just like 2D-CAD.
(2) It corresponded to input and output of DWG file.
(3) Together with major improvement of change area search, processing speed 
    was raised by about 5 times.
(4) Support outline letter display of TTY font.
(5) Support the second level of JIS kanji by vector font.
Ver.10.01 March 6, 2015
(6) Improvement of PDF output.
Ver.10.01 March 10, 2015
(7) Since it was in abnormal condition by Redo and Undo during polyline 
    input of comment, it prevented from Undo, Redo.
Ver.10.01 March 31, 2015
(8) Font of vector font JIS level-2 kanji set was improved.
(9) In polyline input of comment, when it was going to input the next 
    vertex into the same coordinates as previous vertex, buzzer is sounded 
    and the next vertex was ignored.
Ver.10.01 April 6, 2015
(10) Initial output file name of output was always first open file name. 
     When the number of output files was one, it changed into output file name.
(11) File name of main windw title had always become first open file.
     When file currently displayed on the top window was one, it changed
     into the top window file name.
     When file currently displayed on the top Window was multiple, it
     changed into first open file name.
Ver.10.01 April 12, 2015
(12) When "/h input filename" is specified as a starting parameter of 
     Automatic output special edition version, HPGL file output or 
     printer output can be performed.
(13) The following problems were repaired with HPGL output.
     When "ColorNo" was set into "Single" by OpenFile and HPGL file 
     output was carried out, there was no pen selecting command in 
     outputted HPGL file.
     Then, it changed so that pen of file No. might be selected.
     When MC command existed in HPGL file, priority was given to this, 
     and "DrawMode" specified by OpenFile was ignored.
     When PC command existed in HPGL file, priority was given to this, 
     and color in case "ColorNo" specified by OpenFile is "Single" was 
     ignored.
Ver.10.01 April 13, 2015
(14) File containing Bitmap that resolution, width, and height is large 
     was opened, and processing speed when PDF output was carried out 
     was accelerated.

Ver.10.02 May 20, 2015
(1) AutoSelectPaper (A0/A1/A2-/A3/A4, Portrait/Landscape) function was 
    added by printer output.
Ver.10.02 June 15, 2015
(2) With HPGL file output, when Plotter edit button is pushed, HPGL 
    origin position can be selected from "LeftDown of draw area" or 
    "Same of draw origin."
(3) Repair defect of HPGL file output.
(4) Repair display defect of dotted line and dashed line.
Ver.10.02 June 16, 2015
(5) Plotter edit button is pushed and it enabled it to specify arc tolerance
    (Obey input Data, Chord length, Chord angle) with HPGL file output.
Ver.10.02 June 19, 2015
(6) It improved so that initial value (value set up with set pen menu) 
    of color and line width to each pen might be outputted with HPGL 
    file output of HPGL/2 specification.
    If there is no designation of color and line width to pen into input 
    file, this initial value will be used.
(7) With HPGL file output of HPGL specification, it eliminated that command 
    of HPGL/2 was mixed in part.
    And, it changed that font selecting of text was outputted by command 
    of HPGL/2 into command of HPGL.

Ver.10.03 July 19, 2015
(1) It supported to input of SXF file (file extension is P21 and SFC).
(2) Request Input file attribute menu was added.
    Undefined D code information can be confirmed about GERBER file.
    Undefined T code information can be confirmed about NC-Drill file.
(3) It supported to AC (hatching starting point) command of HPGL.
(4) It corresponded to hatching of dotted line and chained line with DXF 
    output of GX-5.
Ver.10.03 July 25, 2015
(5) Information on input file attribute was increased at the time of SXF 
    file input.
(6) It repaired that vertical writing text had fault by SXF file input.
(7) Processing of DV (text route) command except right writing was repaired.

Ver.10.04 August 12, 2015
(1) SXF output functions were added.
(2) Defect of SXF input was repaired.
(3) With DXF output, when there existed image, it repaired abnormal having 
    outputted.
(4) Text of Vector font repaired fault which becomes dotted line and chained 
    line sometimes with DXF and IGES output.
Ver.10.04 September 15, 2015
(5) It supported to Windows10.
Ver.10.04 November 17, 2015
(6) Abnormality display has been improved for arc of very small angle.
(7) In PDF output etc., polygon-ized accuracy of very small circle painting 
    out was raised.
Ver.10.04 November 20, 2015
(8) It enabled it to set up judgment angle of very small arc or circle by 
    "Set"-"Input file"-"Circle and arc judging angle".
Ver.10.04 March 6, 2016
(9) Help explanatory note of change area search was modified.
Ver.10.04 March 16, 2016
(10) Function when "#2 PlotterUnits by 1mm(Step Count)" was changed with 
     Plotter Edit button of HPGL Plotter output was changed.
(11) It repaired that rotation display of file including AC (painting-out 
     start points) command was abnormal.
(12) In the condition that file in which comment Bitmap exists is rotated 
     and displayed, when HPGL Plotter output was carried out, it repaired 
     displaying Bitmap on abnormal position.
Ver.10.04 April 3, 2016
(13) With HPGL Plotter output, it repaired that Up and Down length of 
     dotted line, dashed line, and chained line of comment was abnormal.
Ver.10.04 July 19, 2016
(14) Problem when file with comment created by PloComp before Ver.9.0 is 
     opened was repaired.
Ver.10.04 July 21, 2016
(15) Current update of the description of help was carried out.
Ver.10.04 July 25, 2016
(16) Defect of LA (line attribute) command in case line end and joint 
     shape are except being round was repaired.
(17) "Initial of Line End Shape" of "Set-Line property" dialog was changed 
     into "Shape of line end and joint".
Ver.10.04 September 15, 2016
(18) Depending on PDF creation application, PDF version information may 
     not match notation and entity. When such a PDF file was read, it was 
     not able to read (error code=10000).
     It enabled it to read this.
Ver.10.04 September 23, 2016
(19) When HPGL file was opened in the state of ON of "edit", it repaired 
     that painting-out processing became abnormal.
Ver.10.04 September 30, 2016
(20) When another command (point out menu or icon) was issued without 
     pressing Enter key (end is illustrated) during comment input, it 
     repaired that display was abnormal.
Ver.10.04 October 1, 2016
(21) When another command (point out menu or icon) was issued without 
     pressing Enter key (end is illustrated) during comment input, it 
     repaired that display was abnormal.
(22) Insert comment into file which is not entered.
     And it outputs without displaying.
     Then, there was problem to which comment is not outputted.
     This was repaired.
(23) After output, input comment without displaying.
     Then, there was problem to which color of dragging or rubber band 
     of figure while input becomes strange.
     This was repaired.
Ver.10.04 November 6, 2016
(24) Display command can be issued while comment input.

Ver.10.05 November 24, 2016
(1) When PDF output of plural files is carried out in the state of 
    "Displays in piles", the attribute of layer will enter into PDF file.
    When viewing with PDF viewer, ON/OFF of display in layer unit enables.
    File number of PloComp turns into layer number in PDF file.
(2) With PDF output, "Add PDF note annotation on comment cloud mark 
    closed loop" function was added.
    Attach PDF note annotation on change area automatically by this 
    function, and when keying change report into the PDF note annotation 
    with PDF viewer, use it.
Ver.10.05 November 29, 2016
(3)It enabled it to also choose blank although annotation added by 
   "Add PDF note annotation on comment cloud mark closed loop" function 
   of PDF output was consecutive numbers.
Ver.10.05 December 20, 2016
(4) When Bitmap was in Macro of comment, other figures were displayed 
    under Bitmap and had disappeared.
    This was improved so that other figures might be displayed on Bitmap.
(5) When Macro input of comment was carried out after carrying out 
    various setup, setup after change was not being reflected.
    This was repaired.
(6) It was made to reflect "Ignore PC command" of SetPen in Macro input 
    of comment.
(7) When output drawing size is larger than paper size by preview of 
    Printer-Plotter output, drawing of the right,left,upper and lower 
    position was abnormal.
    This was repaired.
Ver.10.05 December 23, 2016
(8) File of only comment data was opened, and when the number of 
    plotter units set except 40 and carried out HPGL Plotter output, 
    it repaired that output HPGL data became abnormal.
Ver.10.05 January 3, 2017
(9) PayPal fee about licensing fee remittance which user had paid was 
    eliminated.
Ver.10.05 January 9, 2017
(10) When evaluation period goes out, or when uninstalling, function 
     which fills in evaluation result and carries out e mail 
     transmission was added.

Ver.10.06 February 20, 2017
(1) At the time of comment input, function in which it can input 
    after displaying comment property set Dialog and setting property 
    was added.
    ON/OFF of this function can be performed by comment property set Dialog.
(2) It enabled it to issue display command by key while comment input.
Ver.10.06 May 10, 2017
(3) It was ignored when there existed Bitmap which black and white reversed 
    in PDF and EMF input, and it repaired becoming whole surface black.
Ver.10.06 September 27, 2017
(4) Display of FT command of HPGL was improved.
Ver.10.06 January 29, 2018
(5) Fixed abnormally when opening some abnormal files.

Ver.10.07 March 27, 2018
(1) The paper standard (ISO A0-A4, ISO B0-B5, JIS B0-B5, ANSI A-E, ARCH A-E,
    E1) can be set by specifying the paper size of the printer, PDF, TIFF, 
    Bitmap, JPEG, GIF, PNG, PCX, FPX output Dailog.
(2) At "File" - "Create new comment" command, or "Set" - "Comment draw area" 
    command, drawing size can be selected from next paper standard paper size.
    ISO A0-A4, ISO B0-B5, JIS B0-B5, ANSI A-E, ARCH A-E,E1
(3) In the case of automatic paper selection with printer output, when 
    the output drawing size exceeds the maximum paper size that can be
    selected, the largest paper is selected and the output scale is 
    automatically adjusted so that the drawing size matches the paper size.
(4) When selecting automatic paper for output (PDF, TIFF, Bitmap, JPEG, 
    GIF, PNG, PCX, FPX), change the smallest paper selection order as follows.
    Conventional
    A4 landscape    A4 portrait    A3 landscape    A3 portrait
    New
    A4 portrait    A4 landscape    A3 landscape    A3 portrait
(5) The paper size was displayed in the preview window toolbar when 
    previewing with printer output.
(6) By double clicking the status bar of the main window, XY coordinates 
    of HPGL unit (0.025 mm is 1 HPGL unit) are displayed in addition 
    to ordinary XY coordinates.
(7) Opening a number of drawings with different drawing sizes with 
    "Displays in arranges" and previewing the printer output revised 
    the abnormal display.
(8) Fixed the problem that character position shifted under extremely 
    rare conditions.
    Condition: 
    When characters are drawn with multiple LB (label command) without 
    pen movement instruction after LO (label origin command) other 
    than initial value
(9) Under the following conditions, we corrected the fault that black 
    and white color selection was displayed incorrectly.
    Set to black and white
    Data that draws figures while changing colors with PC (pen color 
    designation) command
(10) Fixed an obstacle in which filled figures are not displayed 
    with EMF output.
(11) When multiple drawings were opened with "Displays in arranges" 
    and previewed with HPGL plotter output, the size of the first 
    drawing became all the sizes, and when the second and subsequent 
    drawings were large, it was clipped.
(12) When the special output version of PloComp of automatic output 
    is activated on the command line and the output type changes, 
    the problem that the output condition becomes indefinite unless 
    the same output is made in the dialog mode beforehand was fixed.
Ver.10.07 May 04, 2018
(13) Improved reading accuracy of PDF files.
    PDF reading scale correction is automatically set during installation.
    PDF reading scale correction X, Y can be set in the input file setting.
    We prepared a button which can automatically set PDF reading scale 
    correction X, Y in input file setting.
    PDF reading scale correction can be set automatically on the command line.
(14) Changed the output scale in File - Convert PDF file menu as follows.
    Applied to PS, EPS, XPS, HGL, PCL -> Aplide to PS, EPS, XPS, PCL
    Note: This scale also applies when opening PDF ->
          HGL applies PDF reading scale correction of input file setting Dialog
    Conventionally, the same value was used for Convert PDF file and PDF open, 
    but this time separate memories are memorized.
(15) When the origin of the file was shifted from (0,0), We fixed that 
    only the surface figure displayed without moving the origin.
Ver.10.07 May 08, 2018
(16) When shifting the origin of the file from (0, 0), the following 
    problems were repaired.
    E The position of the surface figure is shifted or not displayed.
    E The position of the hatching shifts.
    E The position of the bitmap shifts.
    E The drawing area is not the minimum area including the drawing area of 
     all files.
    E The drawing area of the file with view data converted to comment is 
     abnormal
(17) Opening the view file, converting it to comment data, double-clicking 
    the view file in the dialog to open the file, and clearing it will 
    result in an error.
(18) Fixed the problem that the mirror does not be applied the hatching 
    angle when DXF, SXF was output with mirror ON.
(19) The accuracy of PDF output was improved.
Ver.10.07 May 24, 2018
(20) Improvement of fine arc filling accuracy with various outputs.
Ver.10.07 Jun 11, 2018
(21) When the resolution was over 45 degrees with CI (circle drawing) command 
    of HPGL, it was drawing with octagon. We changed it to draw with a triangle 
    when the resolution is 120 degrees or more.
Ver. 10.07 June 29, 2018
(22) With "Length measurement between points" and "Length measurement 
    between lines", when the dimension measurement Dialog was displayed, 
    it was pressed without pressing the "Start" button.
    Also, while designating measurement points, display commands other 
    than mouse clicks can be issued.
Ver.10.07 July 19, 2018
(23) Improve not to flicker display when scroll bar is moved with drag 
    mode ON.
(24) When set to display the scroll bar, the problem that the zoom display 
    area and the scroll bar display area do not match partially was fixed.
(25) We adjusted the size of WindowsFont with PDF output.
(26) When determining the change area, conventionally, the same line 
    segment before and after change was recognized as having changed 
    if the start point and the end point are exchanged.
    We improved this to be no change.
Ver.10.07 July 31, 2018
(27) We adjusted the size of WindowsFont with PDF output.
Ver.10.07 August 6, 2018
(28) We adjusted the size of WindowsFont by screen display and image 
    file output.
Ver.10.07 August 10, 2018
(29) The initial color values of pen table No. 3 and 4 are matched with 
    the color table of the comment file.
    When using this table, when converting the view file to the comment file, 
    the pen number of the figure of the comment file becomes the same as 
    the view file.
Ver.10.07 August 16, 2018
(30) Fixed an obstacle that did not display the text color found in 
    "Request-Text" as mark pen color.
(31) When changing the pen table No., the mark pen number is changed so that 
    the mark pen color does not change.

Ver.10.08 October 23, 2018
(1) The following Text comparison mode was added by Request-ChangArea.
     E Image (convert string to image and compare)
     E 1 string (compare row by row) 
     E 1 character (compare 1 character by 1 character)
   PloComp displays the string so that the width of the string becomes 
   the following width.
    String width = (character width + character spacing)  ~ 
                   number of characters - character spacing
   If you set the variable character width font in the Set-Text Menu, 
   for example, the letter "I" has a narrow character width and the 
   letter "W" is wider.
(2) Kanji of HPGL specification is to switch to kanji mode and to use JIS 
    code by LB (Label) command. However, there is data that uses ShiftJIS 
    code in the case of not switching to Kanji mode (1 Byte mode). 
    Therefore, even in such a case, we improved to display Kanji.
(3) When Text size correction was set to something other than 100% with 
    Set-Text, it did not work correction value or position of Text. 
    We improved this.
(4) If Text is on the boundary of the drawing size, influence the drawing 
    area. Conventionally, when "Text size correction" is set to a value 
    other than 100% in Set-Text, when opening a file, Text area was 
    calculated with standard size. This was changed to the corrected size.
(5) In case of combination of DV (horizontal writing, vertical writing 
    character) instruction and LO (designation of left alignment, right 
    alignment, centering of character string) instruction, there was a 
    case where character misalignment occurred. We fixed this.
(6) Check "Edit" in File Open Dialog and open it and display File Open 
    Dialog again, * mark on the layer with comment data did not mark. 
    We fixed it to be attached.
(7) When the Slant angle of Text was other than 0 degree in PDF output, 
    it displayed abnormally. We fixed this.
(8) Fixed a problem that caused a system error if the file extension was 
    not registered when specifying the file name to be opened on the 
    command line.
     E  E  E PloCompAuto compatible automatic output PloComp function for 
          special specification
(9) When selecting the automatic paper selection for various kinds of 
    output and the drawing size of the opened file coincides with the 
    standard paper size, the one larger size was selected. We fixed this.
(10) Some menu shortcut keys did not work. We fixed this.
(11) When inputs DXF file, clockwise circular data was skipped. 
    We fixed this.
(12) It was not corresponded with DXF file input when Text width and 
    Text space were minus (mirror display). Corresponding to this.
(13) Text size at PDF input was adjusted.
Ver.10.08 November 19, 2018
(14) When cloud mark figures are output with HPGL output, they were 
     divided into arc units in the past. This was made into data 
     in which arcs are continuous.
Ver.10.08 December 19, 2018
(15) The following obstacle that occurred from Ver. 10.08 dated 
     October 23, 2018 was repaired.
     When changing the origin of each file from (0, 0) in the file 
     opening dialog etc., the label figure did not move the origin.
Ver.10.08 December 24, 2018
(16) Fixed an error occurred when opening a file according to the 
     condition by correction of Ver. 10.08 (6) dated October 23, 2018.
Ver.10.08 January 2, 2019
(17) Open the file with Edit ON in the file Dialog. 
     After that, we fixed the obstacle which caused error when 
     selecting previously opened file on the file menu.
(18) Select "Display in arranges" in the "Set Display ON/OFF" menu.
    Then, after selecting the comment and selecting the "Com: Display 
    Ploperty" menu, 'Data end!' Is displayed. We fixed this obstacle.

Ver.10.10 January 23, 2019
(1) The following functions were upgraded by drastically updating the 
    PDF reading module.
    * Traditionally, when reading PDF files edited with PDF editing tools 
      such as Acrobat, edited figures were not displayed.
      We made it to display.
    * Text reading processing was adjusted.
    * The clipping process was adjusted.
(2) Processing speed has been greatly improved when multiple file 
    conversion processing is performed at once for the automatic output 
    special specification version.
    It is realized by newly preparing the next command line.
       PloComp.exe /z "batch file name"
    The batch file is a file conversion process of one line at a time, 
    describing the conventional command line parameters, and this is 
    described in plural lines.
(3) Conventionally, when a file is opened with a single color, all the 
    figures including the figure drawn by the background color are drawn 
    in a single color.
    This time, figures drawn by background color are improved to draw 
    with background color.
(4) When character width or character height is minus in reading EMF file, 
    it was not displayed with mirror-on.
    We tried to display with mirror-on.
(5) When arrange display is set and comment is selected and the comment 
    attribute display menu is selected, the problem that nothing is 
    displayed is fixed.
(6) Fixed an error that caused automatic scale correction of PDF file 
    setting by selecting set - input file menu.
(7) Set "Displays in arranges" in the "Set - Display ON/OFF" menu.
    Then, open the file of multiple pages.
    Next, open a file of multiple pages with one Window maximized.
    A system error occurred.
    We fixed this obstacle.
(8) When opening a file with edit ON, the window in the surface was 
    changed from filling to alternate filling.
(9) At the time of EMF output, the character width sometimes became 
    abnormal depending on the situation. We fixed this.
(10) When the origin of Bitmap data is outside the drawing area, the 
    position of the Bitmap is displayed displaced at Plotter output.
    We fixed this.
(11) We modified the garbled character by conditions in HPGL file output.
(12) An error occurred when the width of the drawing size or the height 
    was zero in the image file output. We fixed this.
(13) In DXF, DWG output, polyline error sometimes occurred. We fixed this.
Ver.10.10 February 02 day of 2019
(14) Fixed a problem that an error occurs although files are created by 
   PDF to XPS conversion.
(15) Fixed a problem that PCL conversion from PDF can not be done.
(16) When opening the file in the maximized state for both the Main 
   Window and the Child Window, there was a problem that the maximize, 
   minimize, normalize icons on the upper right of the child window 
   disappeared. We fixed this.
Ver.10.10 March 06, 2019
(17) Added "Display page thumbnail in PDF viewer" function in PDF output.
Ver.10.10 April 26, 2019
(18) Since the HPGL file has no drawing area information, the maximum 
    area of figure is used as the drawing area.
    The "Set""Input File" menu now allows you to select the method for 
    determining the drawing size of the HPGL file from the following.
     * Figure maximum area
     * PS (PlotSize) instruction area. 
       Maximum area of figure without PS instruction.
     * IW (Input Winow) instruction area. 
       Maximum area of figure without IW instruction.
     * IP (ScalePoint) instruction area. 
       Maximum area of figure without IP instruction.
     * Automatic (PS    IW    IP    maximum figure)
    In addition, setting whether to include the origin in the drawing size.
(19) PloComp drawing area (Dis-All area) when reading DXF / DWG file 
    can be selected from figure maximum area or drawing size of 
    DXF / DGW file.
    The PloComp drawing area when reading SXF file is the drawing size of
    the SXF file.
(20) The drawing area of PDF,DXF,SXF output file was made the same as the 
    PloComp drawing area.
(21) Information indicating drawing area is included in data in HPGL 
    file output.
    When this HPGL file is read by PloComp, it is reflected in the 
    drawing area (whole display area) of PloComp.
Ver.10.10 Jun 01, 2019
(22) Fixed the problem of abnormal display when there are multiple 
    Splines according to the condition in DXF file input.
(23) Fixed the problem that the surface becomes abnormal display according 
    to the condition by PDF file input.
(24) In the Set-Display ON/OFF menu, when the display button or the OK 
    button is pressed in Displays in piles, the whole display has been 
    performed conventionally. I changed this to zoom area display.

Ver.10.11 July 17, 2019
(1) A mode was added to set HPGL Pen No. to IGES layer No. in IGES output.
Ver.10.11 August 23, 2019
(2) The following modifications were made to the automatic output special
    specification PloComp.
    When multiple command lines are described on the batch file output 
    command line, the previous command line files are partially 
    overlapped when the command lines on the second and subsequent lines 
    are executed.
Ver.10.11 Oct 01, 2019
(3) When ordering from Japan, the tax of the license fee was changed to 10%.
Ver.10.11 October 19, 2019
(4) When putting the Windows GodMode icon on the desktop, an error 
    occurred at startup. This was repaired.
Ver.10.11 January 14, 2020
(5) Conventionally, free software "Teigha File Converter" has been used 
    for DWG-DXF conversion.
    Open Design Alliance, the copyright holder of "Teigha File Converter",
    has changed it to "ODA File Converter".
    So we responded to this.
    Note: "Teigha File Converter" can be used as it is.
(6) Added support for text format codes (Unicode, MIF, forced line feed) 
    when reading from DWG or DXF.
Ver.10.11 May 18, 2020
(7) DXF, DWG, PDF, and EMF files could not be opened normally when the 
    decimal symbol in the numeric format in the Regional and Language 
    Options of the control panel is other than ".".
    I repaired this.
Ver.10.11 September 12, 2020
(8) When inputting a comment Macro, it has been fixed that it hangs when 
    a file other than the comment file is input.
(9) When you try to open another file or close after entering or editing 
    a comment,'Comment is changed. Save it ?'Dialog is displayed. 
    Changed to display the comment file name to be saved here.
(10) When opening an image file such as a TIFF file with 16 million 
    colors, if ColorNo is set to Sigle, the problem that the specified 
    color is not obtained has been solved.
Ver.10.11 October 01, 2020
(11) Set Window to "Displays in arranges", open multiple files, maximize 
    Window, and the default output file name for various outputs is not 
    the file name displayed in the Window title. So I repaired it.
(12) Fixed that an error is displayed when the window is set to 
    "Displays in arranges", the window is maximized and the window 
    is closed.
(13) Fixed that an error is displayed when the operation of opening 
    the file and closing all windows is repeated.
Ver.10.11 November 15, 2020
(14) Fixed an error in "Search line connection" when the View file 
    drawing area is larger than the comment maximum drawing area. 
    Also, "Search line connection", "Edit" ON to open, and "Convert 
    Connect Line to Comment" command will display a message to scale 
    down and reload the View file.
Ver.10.11 April 01, 2021
(15) When the origin of the file is moved to a position other than
    (0,0) by plotter output, there is a problem that the display
    position of the surface shifts. This was repaired.
(16) In the plotter output, even if the HPGL origin position was set
    to be the same as the drawing origin, there was a problem that
    the position was at the lower left. This was repaired.
(17) When a file containing image data was opened and output to a 
    plotter, there was a problem that the display position was misaligned
    and a large margin was generated.
(18) When a file containing an IW instruction (area clip instruction)
    was read and output to a plotter, there was a problem that the
    clipped area was shifted depending on the output setting conditions.
    This was repaired.

Ver.10.12 April 08, 2021
(1) The drawing origin set in the "Open file" Dialog or the 
    "Drawing origin setting" Dialog has been rounded to 0.025mm even if 
    it is specified in 0.001 mm units.
    This was improved so that it would be in units of 0.001 mm without 
    rounding.
Ver.10.12 July 18, 2021
(2) When opening multiple HPGL files and outputting HPGL Plotter, 
    if there is a PS (drawing size setting) command and image data in 
    the second and subsequent files, the problem that the display 
    position of the image shifts has been fixed.
(3) Fixed the problem that a blank page is displayed in the preview 
    when "Edit" is turned ON or the comment file is opened and 
    "Displays in arranges" is set to output to the plotter printer.
(4) When multiple files were opened and "Displays in arrange" was 
    set for HPGL Plotter output, the output file name was changed 
    to the Active Window file name with the output order number added.
Ver.10.12 December 26, 2021
(5) When outputting to "Windows Printer" with "Output" "Printer, Plotter",
    if "Plot Area" is set to "Zoom Area of Upper Window", the drawing 
    position may shift.

Ver.10.13 December 30, 2021
(1) When "Atypical" was selected for "Paper name" in various outputs, 
    the initial values of "Atypical width" and "Atypical height" were
    298 mm and 210 mm at the first output after starting PloComp.
    The values of "Atypical width" and "Atypical height" were stored 
    at the end of PloComp, and when PloComp was restarted, it was set 
    to the value set at the previous output.
Ver.10.13 January 3, 2022
(2) Changed the text of the button in the "Set Plotter" Dialog of 
    "Output to Printer, Plotter".
    Change the text of the "Set End, Output" button to "Print"
    Change the text of the "Set End" button to "Close"
Ver.10.13 May 2, 2022
(3) The HPGL output has been fixed so that the image is displayed out 
    of alignment.
(4) If the HPGL data has FP (fill) following EP (edge ??line), the system 
    will be abnormal due to comment conversion. This was repaired.
(5) When the HPGL data had continuous EPs (edge ??lines) while changing 
    the pen, the pen width did not change when converted to comments. 
    I made this change the pen width.
(6) When reading a PDF file, the line width of the device-dependent 
    line width pen was displayed as 0.03 mm, but now it is displayed 
    as a line width of 0 mm (minimum width that can be displayed).
(7) Fixed the problem that the characters in the vertical font rotate 
    90 degrees when reading the PDF file.
(8) The temporary processing file that caused an error at the end of 
    the program was deleted.
(9) When a file containing double-byte characters (Kanji) was converted 
    to a comment, the problem of garbled characters was fixed.
(10) Fixed the error that the setting file does not exist when 
     outputting SXF.
(11) When the program is started, the Main Window size and position at 
     the time of the previous termination can be restored. 
     When normalizing from maximizing the Main Window, the child Window 
     sometimes protruded from the Main Window. It was improved so that 
     it would not stick out.
(12) If you turn on "Image down" in "Set" and "Pen", open a file with 
     an image, and output HPGL, the image will shift. This was repaired.
(13) When the entire drawing of the comment file was output by HPGL, 
     the output drawing size was the maximum area of the figure. 
     Changed to the drawing area of the comment file.
(14) The output file name is automatically displayed in various outputs 
     by changing the extension of the input file name. However, 
     if the input file name contains 2 byte characters, an abnormal 
     file name will be displayed. This was repaired.
Ver.10.13 May 9, 2022
(15) The zoom area information shared by all child windows is now retained
     for each child window. In the past, multiple child windows were created,
     the display area was changed for each window to maximize the window, 
     and when the window was switched, the same area was displayed.
(16) When the display angle is other than 0 degrees or the mirror display 
     is set to ON and the "Set" and "Drawing origin" commands are executed, 
     the following message is displayed. Set the display angle to 0 degrees 
     and the mirror display to OFF before executing.
Ver.10.13 June 8, 2022
(17) When all the constituent points of the surface are the same, when 
     opened with Edit OFF, only the outline is drawn and not filled, 
     and when opened with Edit ON, it is painted normally, but there is 
     a problem that it hangs in the comment attribute display. 
     This has been improved.
(18) Added support for alpha blend bitmaps in PDF and EMF files.

Ver.11.00 July 27, 2022
(1) Compatible with Windows 11.
(2) Code signing was added.
    By attaching a code sign, the software distribution source is 
    authenticated, and it is guaranteed that spoofing and content 
    tampering have not been performed.
    Recently, Windows and security check software have tightened 
    security checks, and there are increasing cases of false 
    recognition even though there is no virus. Code signing may 
    reduce false positives.
Ver.11.00 February 10, 2023
(3) Added the following text to Article 2 of "License agreement".
    "This software cannot be operated remotely."
(4) Open a black-and-white TIFF file, select [Set] [Pen], set 
    [Set to Black and White mode] and [output] to ON, 
    and when outputting to PDF, the black and white reversed 
    PDF file will appear. Fixed this bug.

Ver.11.01 March 18, 2023
(1) Fixed the problem that the paper size of the PDF file output 
    by automatic paper selection is slightly deviated from the 
    standard size when the standard size paper is selected for 
    PDF output.
(2) When the left, right, top, and bottom drawing positions of 
    various outputs are set again in one of the outputs, they 
    are reflected in the other outputs.
    However, when the output device for plotter/printer output 
    is switched to HPGL Plotter, the drawing position is automatically 
    set to the lower left. There is a possibility that other output 
    may be performed without noticing the automatic switching.
    Therefore, after outputting to HPGL Plotter, the drawing position 
    is automatically restored.
Ver.11.01 September 15, 2023
(3) Updated the deadline for code signing.
(4) Fixed the following problems in inputting and outputting 
    PDF and EMF files.
   * Display abnormality of Bezier curve when inputting
   * When inputting, display abnormality of POLYPOLYGON (surface) 
     with multiple closed loops
   * Character display error when inputting/outputting a file with 
     characters in vertical writing font with @
(5) Corresponds to vertical writing FONT characters with @ in 
    input/output of HPGL1, DXF, DWG, IGES, and SXF files
(6) Character size adjustment and vertical character error 
    correction when outputting DXF and DWG files
(7) When exporting DXF and DWG files with AutoCAD version GX-5, 
    the font used to be AutoCAD's own Vector Font, but changed to MS Gothic.
(8) Corrected that the character area when selecting individual 
    characters was abnormal when there were multiple lines in the 
    character comment data and the line feed direction was up.
(9) Until now, it was necessary to close the comment attribute 
    display window for each selection. I made it so that the attribute 
    is displayed by selecting it continuously in the open state.
(10) Fixed the following problems in SXF output.
  * Some figures are not output because the layer registration and 
    the layer information of each figure are abnormal.
  * If the origin of the drawing is moved, the figures in the file 
    will be abnormal or will not be output.
  * The figure of the comment data is abnormal or not output.
Ver.11.01 October 20, 2023
(11) Corrected a hang problem when specifying a file type other 
    than "cmt" in Macro input for comments.
Ver.11.01 December 31, 2023
(12) When inputting PDF or EMF files, if "Set" - "InputFile" - 
    "Setup when opening PDF file" - "Delete painting out of white" 
    was turned on, the rectangular filled data was not deleted. 
    I decided to delete this.
Ver.11.01 March 3, 2024
(13) The following HPRTL commands are now supported.
    'ESC%A'(enter PCL mode), 'ESC*rB'(end raster graphics)
    Previously, when opening a file, the image shape of this 
    command was ignored.
Ver.11.01 April 22, 2024
(14) The arc of the comment surface is displayed as a polygon. 
    At that time, I had drawn the arc decomposition angle at 
    5 degrees for the edges and 10 degrees for the fill, so when 
    I enlarged it, the shapes of the peripheral parts did not match.
    Therefore, the arc decomposition angles for edges and f
    ills were unified to 10 degrees.
Ver.11.01 April 29, 2024
(15) Fixed a bug where a white filled rectangle was displayed at 
     the top left of the drawing area when inputting PDF or EMF files.
     This issue is an improvement related to paragraph (12).
     This works regardless of whether "Set"-"InputFile"-
     "Setup when opening PDF file"-"Delete painting out of white" is ON/OFF.
Ver.11.01 May 11, 2024
(16) When inputting a PDF or EMF file, if there was binary data of 
     a raster image figure, there was a problem in which the figure 
     would not be displayed in very rare cases.
     This time, we have revised this.
(17) When inputting PDF or EMF files, it took a long time to open 
     if there were raster image shapes. This has been sped up.

Ver.12.00 December 1, 2024
(1) The quality assurance section of the license agreement has been revised.
(2) If the following conditions are met, the PDF output will be converted 
    to bitmap and output to PDF. 
      A: Displays in piles
      B: Each file has (drawing mode = Merge) and (image data larger than 
         the drawing size) and the number of files is 2 or more
    When multiple image shapes such as bitmaps are layered in PDF, 
    they cannot be displayed in mixed colors (Merge) and are displayed 
    with postscript priority.
    When the results of finding the changed areas of the drawings of 
    two TIFF files using PloComp are output to PDF, only the drawing that 
    was loaded later will be visible.
    This function has been added this time.
(3) In the "Set Input file" dialog, you can now select from the following 
    options for "Data format after reading PDF file (Vector/Image)".
      [1] Vector
      [2] Complex clip: no is Vector / yes is Image
      [3] Image
(4) The routine for reading the coordinates of geometric points when reading
    PDF and EMF files has been completely replaced, and the following 
    improvements have been made.
    - The origin has been changed from the upper left to the lower left.
    - Support for Mapping Mode, which sets the coordinate system of Windows GDI.
    - Scale correction has been performed on EMF file input converted 
      from PDF to EMF.
(5) The following problems have been fixed when reading PDF and EMF files.
    - Circular arcs
    - Rectangles with rounded corners
    - Lines are displayed abnormally when moving the pen up -> drawing text 
      -> moving the pen down -> drawing text
    - Bitmap (STRETCHDIBITS, SETDIBITSTODEVICE) fills the area with black
    - Hatching angles of 45 degrees and 135 degrees are reversed
(6) Support for brushes with bitmap patterns (MR_CREATEDIBPATTERNBRUSHPT,
    EMR_CREATEMONOBRUSH) when importing PDF and EMF files
(7) Surfaces (arcs are decomposed into polygons) with more than 20,000 
    component points could not be displayed. This has been improved so 
    that surfaces with more than 20,000 points can be displayed.
Ver.12.00 December 5, 2024
(8) If the number of closed loops that make up a face exceeded 5,000, 
    the face could not be displayed.
    This has been changed so that the face can be displayed even if 
    the number exceeds 5,000.
(9) Prevented an abnormal termination when the number of fonts exceeds 
    32 during PDF output.
Ver.12.00 February 21, 2025
(10) Comment data would draw the bitmap shape first, then other shapes.
    Therefore, if the bitmap and the filled rectangle were in the same
    position, the bitmap would not be visible.
    So, you selected the "Set" and "Pen" menus and applied the 
    "Turn down image" check ON/OFF function to Comments.
    When ON, the display order is other shapes --> bitmap
    When OFF, the display order is the order of data input
Ver.12.00 February 26, 2025
(11) When outputting PDF, if the TEXT component point exceeds the 
     A0 size, the display of TEXT was restricted. 
     This restriction has been lifted.
Ver.12.00 April 3, 2025
(12) The installation file name has been changed from setup.exe 
     to SetupPloCompE.exe.
Ver.12.00 May 17, 2025
(13) The geometric points of DXF, DWG, and IGES exported figures 
     may be shifted by 0.025 mm. This has been fixed.
Ver.12.00 July 19, 2025
(14) When inputting PDF or EMF, if the bitmap figure meets the 
     following conditions, the display scale becomes abnormal.
     When the bit unit length of the width and height of the bitmap 
     figure matches the HPGL unit length.
     This has been fixed.
Ver. 12.00 January 1, 2026
(15) A function has been added to output PDF files as bitmaps and 
     overlay them when the conditions in (2) dated December 1, 2024 
     are met.
     However, under the following conditions, there was an issue 
     where the shapes in the output PDF would be misaligned, 
     so this has been fixed.
     When loading multiple files, if the drawing origin of the file 
     with the last file number is not (0,0), the output PDF will 
     move to that origin.
Ver. 12.00 January 24, 2026
(16) When "AutoPaperSelect" is selected for "Paper Name" in 
     PDF, Tiff, JPEG, Bitmap, GIF, PNG, PCX, FPX, WMF, PS, FPS, 
     SVG, XPS, or PCL output, the previous help text stated, 
     "If the drawing area is larger than A0, it will be A0 Landscape."
     This was incorrect and has been changed to the following:
     "If the drawing area is larger than A0, the paper size will 
     be the drawing area with the specified "Output Scale" plus 
     the "Paper Margins.""
(17) When "All of Draw" is selected for "Plot Area" in PDF, 
     Tiff, JPEG, Bitmap, GIF, PNG, PCX, FPX, WMF, PS, FPS, 
     SVG, XPS, or PCL output, previously, the lines around the 
     drawing area would disappear during output, so a margin of 
     +1mm was added to the drawing area. However, if you select 
     "Drawing_area+margin" for "Paper name," the output drawing 
     area will be larger than the drawing area.
     For example, if you output input data on A3 paper, the output 
     paper size will be larger than the A3 paper size.
     This time, the +1mm margin has been eliminated. As a result, 
     there are cases where lines on the periphery of the drawing 
     area disappear, but this can be resolved by setting 
     "Paper margin."
     In addition, errors in the calculation of the output paper 
     size have been corrected.
--------------------------------------------------------------------------
                                  [Copyright holder] Isoplotec Corporation
                                       E-Mail ID:isoplotec@isoplotec.co.jp
