MODE	1		// Mord 0/1/2=Microwire/SPI/I2C
CLOCK	1.024KHz	// Clock frequency or cycle.
SPIMODE	3		// Mode of SPI clock. 0/1/2/3
ACCWAIT	1		// The number of waits between access.

							// Define command.
OPCODE	READ	R	00000011	8	8	// READ  = R/W type.=Read  , Code=00000011 , Address bit width.=8 , Data bit width.=8
OPCODE	RDSR	R	00000101	0	8	// RDSR  = R/W type.=Read  , Code=00000101 , Address bit width.=0 , Data bit width.=8
OPCODE	WREN	W	00000110	0	0	// WREN  = R/W type.=Write , Code=00000110 , Address bit width.=0 , Data bit width.=0
OPCODE	WRDI	W	00000100	0	0	// WRDI  = R/W type.=Write , Code=00000100 , Address bit width.=0 , Data bit width.=0
OPCODE	WRSR	W	00000001	0	8	// WRSR  = R/W type.=Write , Code=00000001 , Address bit width.=0 , Data bit width.=8
OPCODE	WRITE	W	00000010	8	8	// WRITE = R/W type.=Write , Code=00000010 , Address bit width.=8 , Data bit width.=8

WREN
WRDI
RDSR	01010101			//                     Data.=01010101
WRSR	10101010			//                     Data.=10101010
WRITE	00110011	11000101	// Address.=00110011 , Data.=11000101
READ	10101100	10100101	// Address.=10101100 , Data.=10100101
RDSR	X101010X			//                     Data.=X101010X
READ	10101100	XXXX0101	// Address.=10101100 , Data.=XXXX0101
