;シリアルチャネル１の構成
;iniserial 1 4 16550
serial 1 push "12345678" 0d 0a

serial 1 init 4 16550

serial 1 push "12345678" 0d 0a
serial 1 pull 
serial 1 pull 10

serial 1 set CTS on
serial 1 set DSR off
serial 1 set RI on
serial 1 set DCD on
serial 1 wait DTR
serial 1 wait RTS
serial 1 wait OUT1
serial 1 wait OUT2

serial 1 pull xx
serial 1 set DCD onn
serial 1 set DC onn
serial 1 probe RTSs
serial 1 probee RTS

